[Version]
Signature="$CHICAGO$"
Class="USB sChip"
provider=%CMPY%  ;This string will be put in registry.
ClassGUID={36FC9E60-C465-1706-8086-444553544016}
LayoutFile=layout.inf
DriverVer=05/18/2001, 1.2.1


[ClassInstall]
Addreg=Class.AddReg

[ClassInstall32]
Addreg=Class32.AddReg

[Class.AddReg]
HKR,,,,%ClassName%
HKR,,Icon,,"-20"

[Class32.AddReg]
HKR,,,,%ClassName%
HKR,,Icon,,"-20"

[Manufacturer]
%MfgName%=NETCOM

[NETCOM]
%USB\VID_5042&PID_ABCD.DeviceDesc%=SCHIP.Dev, USB\VID_5042&PID_ABCD

[PreCopySection]
HKR,,NoSetupUI,,1

[DestinationDirs]
SCHIP.Files.Ext = 10,System32\Drivers
SCHIP.Files.Inf = 10,INF

[SCHIP.Dev]
CopyFiles=SCHIP.Files.Ext, SCHIP.Files.Inf
AddReg=SCHIP.AddReg

[SCHIP.Dev.NT]
CopyFiles=SCHIP.Files.Ext, SCHIP.Files.Inf
AddReg=SCHIP.NT.AddReg

[SCHIP.Dev.NT.Services]
Addservice = SCHIPABCD, 0x00000002, SCHIP.AddService

[SCHIP.AddService]
DisplayName    = %SCHIP.SvcDesc%
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 2                  ; SERVICE_AUTO_START
ErrorControl   = 1                  ; SERVICE_ERROR_NORMAL
ServiceBinary  = %10%\System32\Drivers\schpABCD.sys
LoadOrderGroup = Base

[SCHIP.AddReg]
HKR,,DevLoader,,*ntkern
HKR,,NTMPDriver,,schpABCD.sys
HKR,,UserID,0x00010001,43981
HKR,,EnumPropPages32,,"sysclass.dll,USBEnumPropPages"

[SCHIP.NT.AddReg]
HKR,,DevLoader,,*ntkern
HKR,,NTMPDriver,,schpABCD.sys
HKR,,UserID,0x00010001,43981
HKR,,EnumPropPages32,,"sysclass.dll,USBEnumPropPages"
HKLM,"System\Currentcontrolset\Services\SCHIPABCD","UserID",0x10001,43981

[SCHIP.Files.Ext]
schpABCD.sys

[SCHIP.Files.Inf]
schpABCD.inf

[Strings]
CMPY="NETCOM "
MfgName="NETCOM Shenzhen"
USB\VID_5042&PID_ABCD.DeviceDesc="aa"
SCHIP.SvcDesc="NETCOM USB sChip(ABCD) driver"
ClassName="USB sChip"
InstallDisk="aa Driver Disk"